**■Product Information**

Product Name：19 Inch ODF

Product Model：24C-SC-1U- Type

**■Applications**

 ▶Optical Access Network

▶Data Processing Centers

▶Cable television

▶Local Area Network

▶Coarse Wavelength Division Multiplexer

■Features

▶Design of fixed panel

▶Drawing type structure, convenient construction operation

▶Fit for“19”rack.

▶Suitable for FC,SC,LC,ST,etc

**■Configuration**

|  |  |  |
| --- | --- | --- |
| Item | Specification | Remark |
| Size（mm） | 435\*315\*1U |  |
| Fiber core number | LC Pigtail | 48(DX) |  |
| SC Pigtail | 24（SX） |  |
| Cassette | 1\*24C or 2\*12C or 2\*24C |  |
| Material | Cold-Rolled steel plate |  |
| Thickness of material（mm） | 1.2 |  |
| Weight（KG） | 3.6 |  |
| Color | Black |  |
| Color Number | / |  |
| Operating Temperature（℃） | -40～+65 |  |

**■Optical Parameter**

|  |  |  |
| --- | --- | --- |
| Item | Characteristics | Remarks |
| Pigtail | Fiber Type | G.657A1 |  |
| Length of | 1.5M |  |
| Color | [multicolour](https://fanyi.so.com/# multicolour) |  |
| Insertion Loss | ≤0.3dB |  |
| Return Loss | SM:APC≥60dB,UPC≥50dB |  |
| Repeatability | ≤0.2dB |  |
| Interchange | ≤0.2dB |  |
| Operation Temperature | -30～75℃ |  |
| Relative Humidity | ≤85% |  |

**■Cable Route**



 The branch cable is fused through the

 molten disc in the box and the installed

 cable tail fiber.

 .

**■Accessories**

1. cassette：1\*24C or 2\*12C or 2\*24C
2. Clamps：4 Set.
3. fixing bolts: 4 pcs
4. SC adapters: 24 pcs SC simplex
5. heat shrink: 24pcs